| CMSIS-Driver Version 2.02 Peripheral Interface for Middleware and Application Code

- CMSIS
- CORE
- Driver
- DSP
- RTOS API
- Pack
- SVD

- Main Page
- Usage and Description
- Reference

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Content | Data Structures | Typedefs | Functions
USB Host
USB Host Interface

Driver API for USB Host. More...

## Content
| USBH Port Events
| The USB Host driver generates Port call back events that are notified via the function ARM_USBH_SignalPortEvent.
| USBH Pipe Events
| The USB Host driver generates Pipe call back events that are notified via the function ARM_USBH_SignalPipeEvent.
| USBH Packet Information
| Specify USB packet information used by the function ARM_USBH_PipeTransfer.

## Data Structures
struct | ARM_DRIVER_USBH
| Access structure of USB Host Driver. More...
struct | ARM_USBH_CAPABILITIES
| USB Host Driver Capabilities. More...
struct | ARM_USBH_PORT_STATE
| USB Host Port State. More...

## Typedefs
typedef uint32_t | ARM_USBH_PIPE_HANDLE
| USB Host Pipe Handle.
typedef void(* | ARM_USBH_SignalPortEvent_t )(uint8_t port, uint32_t event)
| Pointer to ARM_USBH_SignalPortEvent : Signal Root HUB Port Event.
typedef void(* | ARM_USBH_SignalPipeEvent_t )(ARM_USBH_PIPE_HANDLE pipe_hndl, uint32_t event)
| Pointer to ARM_USBH_SignalPipeEvent : Signal Pipe Event.

## Functions
ARM_DRIVER_VERSION | ARM_USBH_GetVersion (void)
| Get driver version.
ARM_USBH_CAPABILITIES | ARM_USBH_GetCapabilities (void)
| Get driver capabilities.
int32_t | ARM_USBH_Initialize (ARM_USBH_SignalPortEvent_t cb_port_event, ARM_USBH_SignalPipeEvent_t cb_pipe_event)
| Initialize USB Host Interface.
int32_t | ARM_USBH_Uninitialize (void)
| De-initialize USB Host Interface.
int32_t | ARM_USBH_PowerControl (ARM_POWER_STATE state)
| Control USB Host Interface Power.
int32_t | ARM_USBH_PortVbusOnOff (uint8_t port, bool vbus)
| Root HUB Port VBUS on/off.
int32_t | ARM_USBH_PortReset (uint8_t port)
| Do Root HUB Port Reset.
int32_t | ARM_USBH_PortSuspend (uint8_t port)
| Suspend Root HUB Port (stop generating SOFs).
int32_t | ARM_USBH_PortResume (uint8_t port)
| Resume Root HUB Port (start generating SOFs).
ARM_USBH_PORT_STATE | ARM_USBH_PortGetState (uint8_t port)
| Get current Root HUB Port State.
ARM_USBH_PIPE_HANDLE | ARM_USBH_PipeCreate (uint8_t dev_addr, uint8_t dev_speed, uint8_t hub_addr, uint8_t hub_port, uint8_t ep_addr, uint8_t ep_type, uint16_t ep_max_packet_size, uint8_t ep_interval)
| Create Pipe in System.
int32_t | ARM_USBH_PipeModify (ARM_USBH_PIPE_HANDLE pipe_hndl, uint8_t dev_addr, uint8_t dev_speed, uint8_t hub_addr, uint8_t hub_port, uint16_t ep_max_packet_size)
| Modify Pipe in System.
int32_t | ARM_USBH_PipeDelete (ARM_USBH_PIPE_HANDLE pipe_hndl)
| Delete Pipe from System.
int32_t | ARM_USBH_PipeReset (ARM_USBH_PIPE_HANDLE pipe_hndl)
| Reset Pipe.
int32_t | ARM_USBH_PipeTransfer (ARM_USBH_PIPE_HANDLE pipe_hndl, uint32_t packet, uint8_t *data, uint32_t num)
| Transfer packets through USB Pipe.
uint32_t | ARM_USBH_PipeTransferGetResult (ARM_USBH_PIPE_HANDLE pipe_hndl)
| Get result of USB Pipe transfer.
int32_t | ARM_USBH_PipeTransferAbort (ARM_USBH_PIPE_HANDLE pipe_hndl)
| Abort current USB Pipe transfer.
uint16_t | ARM_USBH_GetFrameNumber (void)
| Get current USB Frame Number.
void | ARM_USBH_SignalPortEvent (uint8_t port, uint32_t event)
| Signal Root HUB Port Event.
void | ARM_USBH_SignalPipeEvent (ARM_USBH_PIPE_HANDLE pipe_hndl, uint32_t event)
| Signal Pipe Event.

## Description

Driver API for USB Host.

## Data Structure Documentation

struct ARM_DRIVER_USBH

Access structure of USB Host Driver.

The functions of the USB Host driver are accessed by function pointers. Refer to Driver Functions for overview information.

Each instance of an USBH provides such an access struct. The instance is indicated by a postfix in the symbol name of the access struct, for example:

- Driver_USBH0 is the name of the access struct of the first instance (no. 0).
- Driver_USBH1 is the name of the access struct of the second instance (no. 1).

A configuration setting in the middleware allows connecting the middleware to a specific driver instance Driver_USBHn. The default is 0, which connects a middleware to the first instance of a driver.

Note
  The struct must remain unchanged.

### Data Fields
ARM_DRIVER_VERSION(* | GetVersion )(void)
| Pointer to ARM_USBH_GetVersion : Get driver version.
ARM_USBH_CAPABILITIES(* | GetCapabilities )(void)
| Pointer to ARM_USBH_GetCapabilities : Get driver capabilities.
int32_t(* | Initialize )(ARM_USBH_SignalPortEvent_t cb_port_event, ARM_USBH_SignalPipeEvent_t cb_pipe_event)
| Pointer to ARM_USBH_Initialize : Initialize USB Host Interface.
int32_t(* | Uninitialize )(void)
| Pointer to ARM_USBH_Uninitialize : De-initialize USB Host Interface.
int32_t(* | PowerControl )(ARM_POWER_STATE state)
| Pointer to ARM_USBH_PowerControl : Control USB Host Interface Power.
int32_t(* | PortVbusOnOff )(uint8_t port, bool vbus)
| Pointer to ARM_USBH_PortVbusOnOff : Root HUB Port VBUS on/off.
int32_t(* | PortReset )(uint8_t port)
| Pointer to ARM_USBH_PortReset : Do Root HUB Port Reset.
int32_t(* | PortSuspend )(uint8_t port)
| Pointer to ARM_USBH_PortSuspend : Suspend Root HUB Port (stop generating SOFs).
int32_t(* | PortResume )(uint8_t port)
| Pointer to ARM_USBH_PortResume : Resume Root HUB Port (start generating SOFs).
ARM_USBH_PORT_STATE(* | PortGetState )(uint8_t port)
| Pointer to ARM_USBH_PortGetState : Get current Root HUB Port State.
ARM_USBH_PIPE_HANDLE(* | PipeCreate )(uint8_t dev_addr, uint8_t dev_speed, uint8_t hub_addr, uint8_t hub_port, uint8_t ep_addr, uint8_t ep_type, uint16_t ep_max_packet_size, uint8_t ep_interval)
| Pointer to ARM_USBH_PipeCreate : Create Pipe in System.
int32_t(* | PipeModify )(ARM_USBH_PIPE_HANDLE pipe_hndl, uint8_t dev_addr, uint8_t dev_speed, uint8_t hub_addr, uint8_t hub_port, uint16_t ep_max_packet_size)
| Pointer to ARM_USBH_PipeModify : Modify Pipe in System.
int32_t(* | PipeDelete )(ARM_USBH_PIPE_HANDLE pipe_hndl)
| Pointer to ARM_USBH_PipeDelete : Delete Pipe from System.
int32_t(* | PipeReset )(ARM_USBH_PIPE_HANDLE pipe_hndl)
| Pointer to ARM_USBH_PipeReset : Reset Pipe.
int32_t(* | PipeTransfer )(ARM_USBH_PIPE_HANDLE pipe_hndl, uint32_t packet, uint8_t *data, uint32_t num)
| Pointer to ARM_USBH_PipeTransfer : Transfer packets through USB Pipe.
uint32_t(* | PipeTransferGetResult )(ARM_USBH_PIPE_HANDLE pipe_hndl)
| Pointer to ARM_USBH_PipeTransferGetResult : Get result of USB Pipe transfer.
int32_t(* | PipeTransferAbort )(ARM_USBH_PIPE_HANDLE pipe_hndl)
| Pointer to ARM_USBH_PipeTransferAbort : Abort current USB Pipe transfer.
uint16_t(* | GetFrameNumber )(void)
| Pointer to ARM_USBH_GetFrameNumber : Get current USB Frame Number.

#### Field Documentation

ARM_USBH_CAPABILITIES(* GetCapabilities)(void)

Pointer to ARM_USBH_GetCapabilities : Get driver capabilities.

uint16_t(* GetFrameNumber)(void)

Pointer to ARM_USBH_GetFrameNumber : Get current USB Frame Number.

ARM_DRIVER_VERSION(* GetVersion)(void)

Pointer to ARM_USBH_GetVersion : Get driver version.

int32_t(* Initialize)(ARM_USBH_SignalPortEvent_t cb_port_event, ARM_USBH_SignalPipeEvent_t cb_pipe_event)

Pointer to ARM_USBH_Initialize : Initialize USB Host Interface.

ARM_USBH_PIPE_HANDLE(* PipeCreate)(uint8_t dev_addr, uint8_t dev_speed, uint8_t hub_addr, uint8_t hub_port, uint8_t ep_addr, uint8_t ep_type, uint16_t ep_max_packet_size, uint8_t ep_interval)

Pointer to ARM_USBH_PipeCreate : Create Pipe in System.

int32_t(* PipeDelete)(ARM_USBH_PIPE_HANDLE pipe_hndl)

Pointer to ARM_USBH_PipeDelete : Delete Pipe from System.

int32_t(* PipeModify)(ARM_USBH_PIPE_HANDLE pipe_hndl, uint8_t dev_addr, uint8_t dev_speed, uint8_t hub_addr, uint8_t hub_port, uint16_t ep_max_packet_size)

Pointer to ARM_USBH_PipeModify : Modify Pipe in System.

int32_t(* PipeReset)(ARM_USBH_PIPE_HANDLE pipe_hndl)

Pointer to ARM_USBH_PipeReset : Reset Pipe.

int32_t(* PipeTransfer)(ARM_USBH_PIPE_HANDLE pipe_hndl, uint32_t packet, uint8_t *data, uint32_t num)

Pointer to ARM_USBH_PipeTransfer : Transfer packets through USB Pipe.

int32_t(* PipeTransferAbort)(ARM_USBH_PIPE_HANDLE pipe_hndl)

Pointer to ARM_USBH_PipeTransferAbort : Abort current USB Pipe transfer.

uint32_t(* PipeTransferGetResult)(ARM_USBH_PIPE_HANDLE pipe_hndl)

Pointer to ARM_USBH_PipeTransferGetResult : Get result of USB Pipe transfer.

ARM_USBH_PORT_STATE(* PortGetState)(uint8_t port)

Pointer to ARM_USBH_PortGetState : Get current Root HUB Port State.

int32_t(* PortReset)(uint8_t port)

Pointer to ARM_USBH_PortReset : Do Root HUB Port Reset.

int32_t(* PortResume)(uint8_t port)

Pointer to ARM_USBH_PortResume : Resume Root HUB Port (start generating SOFs).

int32_t(* PortSuspend)(uint8_t port)

Pointer to ARM_USBH_PortSuspend : Suspend Root HUB Port (stop generating SOFs).

int32_t(* PortVbusOnOff)(uint8_t port, bool vbus)

Pointer to ARM_USBH_PortVbusOnOff : Root HUB Port VBUS on/off.

int32_t(* PowerControl)(ARM_POWER_STATE state)

Pointer to ARM_USBH_PowerControl : Control USB Host Interface Power.

int32_t(* Uninitialize)(void)

Pointer to ARM_USBH_Uninitialize : De-initialize USB Host Interface.

struct ARM_USBH_CAPABILITIES

USB Host Driver Capabilities.

A USB Host driver can be implemented with different capabilities. The bitfield members of this struct encode the capabilities implemented by this driver.

Returned by:

- ARM_USBH_GetCapabilities

Note
  The struct must remain unchanged.

Data Fields
uint32_t | auto_split: 1 | Automatic SPLIT packet handling.
uint32_t | event_connect: 1 | Signal Connect event.
uint32_t | event_disconnect: 1 | Signal Disconnect event.
uint32_t | event_overcurrent: 1 | Signal Overcurrent event.
uint32_t | port_mask: 15 | Root HUB available Ports Mask.

struct ARM_USBH_PORT_STATE

USB Host Port State.

This structure stores information about the state of the USB Host Port. The bitfields encode whether a device is connected to the port, if port overcurrent is detected and the port speed.

Returned by:

- ARM_USBH_PortGetState

Data Fields
uint32_t | connected: 1 | USB Host Port connected flag.
uint32_t | overcurrent: 1 | USB Host Port overcurrent flag.
uint32_t | speed: 2 | USB Host Port speed setting (ARM_USB_SPEED_xxx)

## Typedef Documentation

uint32_t ARM_USBH_PIPE_HANDLE

USB Host Pipe Handle.

Each pipe is identified through a unique number, which is created by the function ARM_USBH_PipeCreate.

Parameter for:

- ARM_USBH_PipeModify, ARM_USBH_PipeDelete, ARM_USBH_PipeReset, ARM_USBH_PipeTransfer, ARM_USBH_PipeTransferGetResult, ARM_USBH_PipeTransferAbort, ARM_USBH_SignalPipeEvent

Retruned by:

- ARM_USBH_PipeCreate

ARM_USBH_SignalPipeEvent_t

Pointer to ARM_USBH_SignalPipeEvent : Signal Pipe Event.

Provides the typedef for the callback function ARM_USBH_SignalPipeEvent.

Parameter for:

- ARM_USBH_Initialize

ARM_USBH_SignalPortEvent_t

Pointer to ARM_USBH_SignalPortEvent : Signal Root HUB Port Event.

Provides the typedef for the callback function ARM_USBH_SignalPortEvent.

Parameter for:

- ARM_USBH_Initialize

## Function Documentation

ARM_USBH_CAPABILITIES ARM_USBH_GetCapabilities | ( | void |  | ) |

Get driver capabilities.

Returns
  ARM_USBH_CAPABILITIES

Retrieves information about capabilities in this driver implementation. The bitfield members of the struct ARM_USBH_CAPABILITIES encode various capabilities, for example available HUB ports or if the hardware can generate signal events using the ARM_USBH_SignalPortEvent callback function.

Example:

extern ARM_DRIVER_USBH Driver_USBH0;
ARM_DRIVER_USBH *drv_info;
void read_capabilities (void) {
ARM_USBH_CAPABILITIES drv_capabilities;
drv_info = &Driver_USBH0;
drv_capabilities = drv_info->GetCapabilities ();
// interrogate capabilities
}

uint16_t ARM_USBH_GetFrameNumber | ( | void |  | ) |

Get current USB Frame Number.

Returns
  Frame Number

Retrieves the sequential 11-bit frame number of the last Start of Frame (SOF) packet.

ARM_DRIVER_VERSION ARM_USBH_GetVersion | ( | void |  | ) |

Get driver version.

Returns
  ARM_DRIVER_VERSION

Returns version information of the driver implementation in ARM_DRIVER_VERSION

- API version is the version of the CMSIS-Driver specification used to implement this driver.
- Driver version is source code version of the actual driver implementation.

Example:

extern ARM_DRIVER_USBH Driver_USBH0;
ARM_DRIVER_USBH *drv_info;
void setup_usbh (void) {
ARM_DRIVER_VERSION version;
drv_info = &Driver_USBH0;
version = drv_info->GetVersion ();
if (version.api < 0x10A) { // requires at minimum API version 1.10 or higher
// error handling
return;
}
}

int32_t ARM_USBH_Initialize | ( | ARM_USBH_SignalPortEvent_t | cb_port_event,
|  | ARM_USBH_SignalPipeEvent_t | cb_pipe_event
| ) |  |

Initialize USB Host Interface.

Parameters

  [in] | cb_port_event | Pointer to ARM_USBH_SignalPortEvent
  [in] | cb_pipe_event | Pointer to ARM_USBH_SignalPipeEvent

Returns
  Status Error Codes

The function initializes the USB Host interface. It is called when the middleware component starts operation.

The function performs the following operations:

- Initializes the resources needed for the USBH interface.
- Registers the ARM_USBH_SignalPortEvent callback function.
- Registers the ARM_USBH_SignalPipeEvent callback function.

The parameter cb_port_event is a pointer to the ARM_USBH_SignalPortEvent callback function; use a NULL pointer when no port callback signals are required.

The parameter cb_pipe_event is a pointer to the ARM_USBH_SignalPipeEvent callback function.

Example:

- see USB Host Interface - Driver Functions

ARM_USBH_PIPE_HANDLE ARM_USBH_PipeCreate | ( | uint8_t | dev_addr,
|  | uint8_t | dev_speed,
|  | uint8_t | hub_addr,
|  | uint8_t | hub_port,
|  | uint8_t | ep_addr,
|  | uint8_t | ep_type,
|  | uint16_t | ep_max_packet_size,
|  | uint8_t | ep_interval
| ) |  |

Create Pipe in System.

Parameters

  [in] | dev_addr | Device Address
  [in] | dev_speed | Device Speed
  [in] | hub_addr | Hub Address
  [in] | hub_port | Hub Port
  [in] | ep_addr | Endpoint Address ep_addr.0..3: Address ep_addr.7: Direction
  [in] | ep_type | Endpoint Type (ARM_USB_ENDPOINT_xxx)
  [in] | ep_max_packet_size | Endpoint Maximum Packet Size
  [in] | ep_interval | Endpoint Polling Interval

Returns
  Pipe Handle ARM_USBH_PIPE_HANDLE

Creates pipe for transfers (allocates required resources and configures the pipe).

The parameters specify pipe information (connection between host and device endpoint):

- device: address and speed
- hub (optional): hub address and number of the hub port to which the device is connected
- endpoint: address, type, maximum packet size and polling interval

The function returns an pipe handle that is used for all subsequent operations on that pipe. In case of errors an invalid handle (NULL) is returned.

int32_t ARM_USBH_PipeDelete | ( | ARM_USBH_PIPE_HANDLE | pipe_hndl | ) |

Delete Pipe from System.

Parameters

  [in] | pipe_hndl | Pipe Handle

Returns
  Status Error Codes

Deletes pipe that was created with ARM_USBH_PipeCreate (deactivates the pipe and releases used resources).

int32_t ARM_USBH_PipeModify | ( | ARM_USBH_PIPE_HANDLE | pipe_hndl,
|  | uint8_t | dev_addr,
|  | uint8_t | dev_speed,
|  | uint8_t | hub_addr,
|  | uint8_t | hub_port,
|  | uint16_t | ep_max_packet_size
| ) |  |

Modify Pipe in System.

Parameters

  [in] | pipe_hndl | Pipe Handle
  [in] | dev_addr | Device Address
  [in] | dev_speed | Device Speed
  [in] | hub_addr | Hub Address
  [in] | hub_port | Hub Port
  [in] | ep_max_packet_size | Endpoint Maximum Packet Size

Returns
  Status Error Codes

Modifies pipe configuration that was created with ARM_USBH_PipeCreate.

int32_t ARM_USBH_PipeReset | ( | ARM_USBH_PIPE_HANDLE | pipe_hndl | ) |

Reset Pipe.

Parameters

  [in] | pipe_hndl | Pipe Handle

Returns
  Status Error Codes

This function is used to clear Halt condition and reset data toggle on the specified pipe.

int32_t ARM_USBH_PipeTransfer | ( | ARM_USBH_PIPE_HANDLE | pipe_hndl,
|  | uint32_t | packet,
|  | uint8_t * | data,
|  | uint32_t | num
| ) |  |

Transfer packets through USB Pipe.

Parameters

  [in] | pipe_hndl | Pipe Handle
  [in] | packet | Packet information
  [in] | data | Pointer to buffer with data to send or for data to receive
  [in] | num | Number of data bytes to transfer

Returns
  Status Error Codes

This function is used to generate packets in order to send data to or receive data from USB Endpoint.

The function specifies the buffer for data to read or with data to write and the number of bytes to transfer. It also specifies USBH Packet Information with parameter packet.

The function is non-blocking and returns as soon as the driver starts the operation on the specified pipe. During the operation it is not allowed to call this function again on the same pipe. Also the data buffer must stay allocated and the contents of data must not be modified.

Operation is completed when the the requested number of data bytes have been transfered and is indicated with ARM_USBH_EVENT_TRANSFER_COMPLETE event. It can also finish earlier on reception of different handshake tokens which are also indicated through USBH Pipe Events.

Transfer operation can be aborted by calling ARM_USBH_PipeTransferAbort.

int32_t ARM_USBH_PipeTransferAbort | ( | ARM_USBH_PIPE_HANDLE | pipe_hndl | ) |

Abort current USB Pipe transfer.

Parameters

  [in] | pipe_hndl | Pipe Handle

Returns
  Status Error Codes

This function is used to abort active pipe transfer started by ARM_USBH_PipeTransfer.

uint32_t ARM_USBH_PipeTransferGetResult | ( | ARM_USBH_PIPE_HANDLE | pipe_hndl | ) |

Get result of USB Pipe transfer.

Parameters

  [in] | pipe_hndl | Pipe Handle

Returns
  number of successfully transfered data bytes

Returns the number of successfully transferred data bytes started by ARM_USBH_PipeTransfer operation.

ARM_USBH_PORT_STATE ARM_USBH_PortGetState | ( | uint8_t | port | ) |

Get current Root HUB Port State.

Parameters

  [in] | port | Root HUB Port Number

Returns
  Port State ARM_USBH_PORT_STATE

Retrieves the current state of the specified port.

int32_t ARM_USBH_PortReset | ( | uint8_t | port | ) |

Do Root HUB Port Reset.

Parameters

  [in] | port | Root HUB Port Number

Returns
  Status Error Codes

Executes reset signalling on the specified port.

int32_t ARM_USBH_PortResume | ( | uint8_t | port | ) |

Resume Root HUB Port (start generating SOFs).

Parameters

  [in] | port | Root HUB Port Number

Returns
  Status Error Codes

Resumes USB signaling on the specified port.

int32_t ARM_USBH_PortSuspend | ( | uint8_t | port | ) |

Suspend Root HUB Port (stop generating SOFs).

Parameters

  [in] | port | Root HUB Port Number

Returns
  Status Error Codes

Suspends USB signaling on the specified port.

int32_t ARM_USBH_PortVbusOnOff | ( | uint8_t | port,
|  | bool | vbus
| ) |  |

Root HUB Port VBUS on/off.

Parameters

  [in] | port | Root HUB Port Number
  [in] | vbus | false VBUS off true VBUS on

Returns
  Status Error Codes

Allows you to control the VBUS signal of the specified port.

int32_t ARM_USBH_PowerControl | ( | ARM_POWER_STATE | state | ) |

Control USB Host Interface Power.

Parameters

  [in] | state | Power state

Returns
  Status Error Codes

Allows you to control the power modes of the USB Host interface.

void ARM_USBH_SignalPipeEvent | ( | ARM_USBH_PIPE_HANDLE | pipe_hndl,
|  | uint32_t | event
| ) |  |

Signal Pipe Event.

Parameters

  [in] | pipe_hndl | Pipe Handle
  [in] | event | USBH Pipe Events

Returns
  none

The function ARM_USBH_SignalPipeEvent notifies the application of the USBH Pipe Events and it is registered by the function ARM_USBH_Initialize.

The argument pipe_hndl specifies the pipe handle.

The argument event represents the notification mask of the events. Each event is coded in a separate bit and therefore it is possible to signal multiple events in the event call back function. The following call back notifications are generated:

Bit | Event | Description
--- | --- | ---
0 | ARM_USBH_EVENT_TRANSFER_COMPLETE | Occurs after all the data has been transferred without errors.
1 | ARM_USBH_EVENT_HANDSHAKE_NAK | Occurs when NAK Handshake is received before all the data is transferred.
2 | ARM_USBH_EVENT_HANDSHAKE_NYET | Occurs when NYET Handshake is received before all the data is transferred.
3 | ARM_USBH_EVENT_HANDSHAKE_MDATA | Occurs when MDATA Handshake is received before all the data is transferred.
4 | ARM_USBH_EVENT_HANDSHAKE_STALL | Occurs when STALL Handshake is received before all the data is transferred.
5 | ARM_USBH_EVENT_HANDSHAKE_ERR | Occurs when ERR Handshake is received before all the data is transferred.
6 | ARM_USBH_EVENT_BUS_ERROR | Occurs when bus error is detected before all the data is transferred.

void ARM_USBH_SignalPortEvent | ( | uint8_t | port,
|  | uint32_t | event
| ) |  |

Signal Root HUB Port Event.

Parameters

  [in] | port | Root HUB Port Number
  [in] | event | USBH Port Events

Returns
  none

The function ARM_USBH_SignalPortEvent notifies the application of the USBH Port Events and it is registered by the function ARM_USBH_Initialize. The function ARM_USBH_GetCapabilities returns information about the implemented optional events in a driver.

The argument port specifies the root hub port number.

The argument event represents the notification mask of the events. Each event is coded in a separate bit and therefore it is possible to signal multiple events in the event call back function. The following call back notifications are generated:

Bit | Event | Description
--- | --- | ---
0 | ARM_USBH_EVENT_CONNECT | Occurs when USB Device connects to the Host.
1 | ARM_USBH_EVENT_DISCONNECT | Occurs when USB Device disconnects from the Host.
2 | ARM_USBH_EVENT_OVERCURRENT | Occurs when USB Overcurrent it detected.
3 | ARM_USBH_EVENT_RESET | Occurs when USB Reset is completed after calling ARM_USBH_PortReset.
4 | ARM_USBH_EVENT_SUSPEND | Occurs when USB Suspend is detected.
5 | ARM_USBH_EVENT_RESUME | Occurs when USB Resume is detected.
6 | ARM_USBH_EVENT_REMOTE_WAKEUP | Occurs when USB Remote wakeup is detected.

int32_t ARM_USBH_Uninitialize | ( | void |  | ) |

De-initialize USB Host Interface.

Returns
  Status Error Codes

The function ARM_USBH_Uninitialize de-initializes the resources of USB Host interface.

It is called when the middleware component stops operation and releases the software resources used by the interface.