| CMSIS-RTOS RTX Version 4.75 CMSIS-RTOS RTX: Real-Time Operating System for Cortex-M processor-based devices

- RTX

- Main Page
- Usage and Description
- Reference

Using CMSIS-RTOS RTX

Example projects using CMSIS-RTOS RTX are available for various development boards. To make use of these examples, you need to install a Device Family Pack in µVision and use Pack Installer to open a CMSIS-RTOS Blinky project. If you wish to start a CMSIS-RTOS RTX from scratch, follow these steps:

- Create a new project and select a device.

- In the Manage Run-Time Environment window that opens, select CMSIS::CORE and CMSIS::RTOS (API)::Keil RTX. If the Validation Output requires other components to be present, try to use the Resolve button. Click OK:

- In the Project window, you will see the files that have been automatically added to you project, such as RTX_Conf_CM.c and the system and startup files:

- You can add template files to the project by right-clicking on Source Group 1 and selecting Add New Item to 'Source Group 1'. In the new window, click on User Code Template. On the right-hand side you will see all available template files for CMSIS-RTOS RTX: