| CMSIS-Driver Version 2.02 Peripheral Interface for Middleware and Application Code

- CMSIS
- CORE
- Driver
- DSP
- RTOS API
- Pack
- SVD

- Main Page
- Usage and Description
- Reference

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Macros
NAND Sequence Execution Codes
NAND Interface

Specify execution codes. More...

## Macros
#define | ARM_NAND_CODE_SEND_CMD1 (1UL << 17)
| Send Command 1.
#define | ARM_NAND_CODE_SEND_ADDR_COL1 (1UL << 18)
| Send Column Address 1.
#define | ARM_NAND_CODE_SEND_ADDR_COL2 (1UL << 19)
| Send Column Address 2.
#define | ARM_NAND_CODE_SEND_ADDR_ROW1 (1UL << 20)
| Send Row Address 1.
#define | ARM_NAND_CODE_SEND_ADDR_ROW2 (1UL << 21)
| Send Row Address 2.
#define | ARM_NAND_CODE_SEND_ADDR_ROW3 (1UL << 22)
| Send Row Address 3.
#define | ARM_NAND_CODE_INC_ADDR_ROW (1UL << 23)
| Auto-increment Row Address.
#define | ARM_NAND_CODE_WRITE_DATA (1UL << 24)
| Write Data.
#define | ARM_NAND_CODE_SEND_CMD2 (1UL << 25)
| Send Command 2.
#define | ARM_NAND_CODE_WAIT_BUSY (1UL << 26)
| Wait while R/Bn busy.
#define | ARM_NAND_CODE_READ_DATA (1UL << 27)
| Read Data.
#define | ARM_NAND_CODE_SEND_CMD3 (1UL << 28)
| Send Command 3.
#define | ARM_NAND_CODE_READ_STATUS (1UL << 29)
| Read Status byte and check FAIL bit (bit 0)

## Description

Specify execution codes.

The defines can be used in the function ARM_NAND_ExecuteSequence for the parameter code.

## Macro Definition Documentation

#define ARM_NAND_CODE_INC_ADDR_ROW (1UL << 23)

Auto-increment Row Address.

#define ARM_NAND_CODE_READ_DATA (1UL << 27)

Read Data.

#define ARM_NAND_CODE_READ_STATUS (1UL << 29)

Read Status byte and check FAIL bit (bit 0)

#define ARM_NAND_CODE_SEND_ADDR_COL1 (1UL << 18)

Send Column Address 1.

#define ARM_NAND_CODE_SEND_ADDR_COL2 (1UL << 19)

Send Column Address 2.

#define ARM_NAND_CODE_SEND_ADDR_ROW1 (1UL << 20)

Send Row Address 1.

#define ARM_NAND_CODE_SEND_ADDR_ROW2 (1UL << 21)

Send Row Address 2.

#define ARM_NAND_CODE_SEND_ADDR_ROW3 (1UL << 22)

Send Row Address 3.

#define ARM_NAND_CODE_SEND_CMD1 (1UL << 17)

Send Command 1.

#define ARM_NAND_CODE_SEND_CMD2 (1UL << 25)

Send Command 2.

#define ARM_NAND_CODE_SEND_CMD3 (1UL << 28)

Send Command 3.

#define ARM_NAND_CODE_WAIT_BUSY (1UL << 26)

Wait while R/Bn busy.

#define ARM_NAND_CODE_WRITE_DATA (1UL << 24)

Write Data.