| CMSIS-Driver Version 2.02 Peripheral Interface for Middleware and Application Code

- CMSIS
- CORE
- Driver
- DSP
- RTOS API
- Pack
- SVD

- Main Page
- Usage and Description
- Reference

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Structures | Macros | Typedefs
Driver_USBD.h File Reference

## Data Structures
struct | ARM_USBD_STATE
| USB Device State. More...
struct | ARM_USBD_CAPABILITIES
| USB Device Driver Capabilities. More...
struct | ARM_DRIVER_USBD
| Access structure of the USB Device Driver. More...

## Macros
#define | ARM_USBD_API_VERSION ARM_DRIVER_VERSION_MAJOR_MINOR(2,01) /* API version */
#define | ARM_USBD_EVENT_VBUS_ON (1UL << 0)
| USB Device VBUS On.
#define | ARM_USBD_EVENT_VBUS_OFF (1UL << 1)
| USB Device VBUS Off.
#define | ARM_USBD_EVENT_RESET (1UL << 2)
| USB Reset occurred.
#define | ARM_USBD_EVENT_HIGH_SPEED (1UL << 3)
| USB switch to High Speed occurred.
#define | ARM_USBD_EVENT_SUSPEND (1UL << 4)
| USB Suspend occurred.
#define | ARM_USBD_EVENT_RESUME (1UL << 5)
| USB Resume occurred.
#define | ARM_USBD_EVENT_SETUP (1UL << 0)
| SETUP Packet.
#define | ARM_USBD_EVENT_OUT (1UL << 1)
| OUT Packet(s)
#define | ARM_USBD_EVENT_IN (1UL << 2)
| IN Packet(s)

## Typedefs
typedef void(* | ARM_USBD_SignalDeviceEvent_t )(uint32_t event)
| Pointer to ARM_USBD_SignalDeviceEvent : Signal USB Device Event.
typedef void(* | ARM_USBD_SignalEndpointEvent_t )(uint8_t ep_addr, uint32_t event)
| Pointer to ARM_USBD_SignalEndpointEvent : Signal USB Endpoint Event.

## Macro Definition Documentation

#define ARM_USBD_API_VERSION ARM_DRIVER_VERSION_MAJOR_MINOR(2,01) /* API version */