| CMSIS-Driver Version 2.02 Peripheral Interface for Middleware and Application Code

- CMSIS
- CORE
- Driver
- DSP
- RTOS API
- Pack
- SVD

- Main Page
- Usage and Description
- Reference

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Content
MCI Control Codes
MCI Interface

Configure and control the MCI using the ARM_MCI_Control. More...

## Content
| MCI Controls
| Configure and control the MCI interface.
| MCI Bus Speed Mode
| Specify the bus speed mode.
| MCI Bus Data Width
| Specify the data bus width.
| MCI CMD Line Mode
| Specify the CMD line mode (Push-Pull or Open Drain).
| MCI Driver Strength
| Specify the driver strength.

## Description

Configure and control the MCI using the ARM_MCI_Control.

Many parameters of the MCI driver are configured using the ARM_MCI_Control function.

The various MCI control codes define:

- MCI Controls configures and controls the MCI interface
- MCI Bus Speed Mode specifies the bus speed mode
- MCI Bus Data Width specifies the data bus width
- MCI CMD Line Mode specifies the CMD line mode
- MCI Driver Strength specifies the driver strength

Refer to the function ARM_MCI_Control for further details.