| CMSIS-SVD Version 1.2 CMSIS System View Description

- CMSIS
- CORE
- Driver
- DSP
- RTOS API
- Pack
- SVD

- Main Page
- Usage and Description
- Reference

CPU Section (New)
SVD Extension in Version 1.1 and 1.2

The CPU section describes the processor included in the microcontroller device. This section is mandatory if the SVD file shall be used for the device header file generation.

    <cpu>
        <name>cpuNameType</name>
        <revision>revisionType</revision>
        <endian>endianType</endian>
        <mpuPresent>xs:boolean</mpuPresent>
        <fpuPresent>xs:boolean</fpuPresent>
        <fpuDP>xs:boolean</fpuDP>
        <icachePresent>xs:boolean</icachePresent>
        <dcachePresent>xs:boolean</dcachePresent>
        <itcmPresent>xs:boolean</itcmPresent>
        <dtcmPresent>xs:boolean</dtcmPresent>
        <vtorPresent>xs:boolean</vtorPresent>
        <nvicPrioBits>scaledNonNegativeInteger</nvicPrioBits>
        <vendorSystickConfig>xs:boolean</vendorSystickConfig>
    </cpu>

Element Name | Description | Type | Occurrence
--- | --- | --- | ---
name | The predefined tokens are: CM0: ARM Cortex-M0 CM0PLUS: ARM Cortex-M0+ CM3: ARM Cortex-M3 CM4: ARM Cortex-M4 CM7: ARM Cortex-M7 SC000: ARM Secure Core SC000 SC300: ARM Secure Core SC300 other: other processor architectures | cpuNameType | 1..1
revisionType | Defines the HW revision of the processor. The defined version format is rNpM (N,M = [0 - 9]). | revisionType | 1..1
endian | Defines the endianess of the processor being one of: little: little endian memory (least significant byte gets allocated at the lowest address). big: byte invariant big endian data organization (most significant byte gets allocated at the lowest address). selectable: little and big endian are configurable for the device and become active after the next reset. other: the endianess is neither little nor big endian. | endianType | 1..1
mpuPresent | Indicates that the processor is equipped with a memory protection unit (MPU). This tag is either set to true or false, 1 or 0. | boolean | 1..1
fpuPresent | Indicates that the processor is equipped with a hardware floating point unit (FPU). Cortex-M4 and Cortex-M7 are the only available Cortex-M processor with an optional FPU. This tag is either set to true or false, 1 or 0. | boolean | 1..1
fpuDP | Indicates that the processor is equipped with a double precision floating point unit. Flag is only valid if fpuPresent is set true. Cortex-M7 is currently the only Cortex-M processor available with a double precision floating point unit. | boolean | 0..1
icachePresent | Indicates that the processor has an instruction cache. Note: only an option for Cortex-M7 based devices. | 0..1
dcachePresent | Indicates that the processor has an data cache. Note: only an option for Cortex-M7 based devices. | 0..1
itcmPresent | Indicates that the processor has an instruction tightly coupled memory. Note: only an option for Cortex-M7 based devices. | 0..1
dtcmPresent | Indicates that the processor has an data tightly coupled memory. Note: only an option for Cortex-M7 based devices. | 0..1
vtorPresent | This is an optional flag used for the Cortex-M0+ based devices only. It indicates whether the Vector Table Offset Register (VTOR) is implemented in the Cortex-M0+ device or not. This tag is either set to true or false, 1 or 0. If it is not specified VTOR is assumed to be present. | boolean | 1..1
nvicPrioBits | Defines the number of bits that are available in the Nested Vectored Interrupt Controller (NVIC) for configuring the priority. | scaledNonNegativeInteger | 1..1
vendorSystickConfig | Indicates whether the processor implements a vendor-specific System Tick Timer. If false, then the ARM defined System Tick Timer is available. If true, then a vendor-specific System Tick Timer must be implemented. This tag is either set to true or false, 1 or 0. | boolean | 1..1

# Example:

...
<cpu>
<name>CM7</name>
<revision>r0p0</revision>
<endian>little</endian>
<mpuPresent>true</mpuPresent>
<!-- has double precision FPU -->
<fpuPresent>true</fpuPresent>
<fpuDP>true</fpuDP>
<!-- has instruction and data cache -->
<icachePresent>true</icachePresent>
<dcachePresent>true</dcachePresent>
<!-- has no instruction nor data tighly coupled memory -->
<itcmPresent>false</itcmPresent>
<dtcmPresent>false</dtcmPresent>
<nvicPrioBits>4</nvicPrioBits>
<vendorSystickConfig>false</vendorSystickConfig>
</cpu>
...

This example describes a Cortex-M4 core of HW revision r0p0, with fixed little endian memory scheme, including Memory Protection Unit and hardware Floating Point Unit. The Nested Vectored Interrupt Controller uses 4 bits for configuring the priority of an interrupt. It is equipped with the standard System Tick Timer as defined by ARM.