| CMSIS-CORE Version 4.00 CMSIS-CORE support for Cortex-M processor-based devices

- CMSIS
- CORE
- Driver
- DSP
- RTOS API
- Pack
- SVD

- Main Page
- Usage and Description
- Reference

All Data Structures Files Functions Variables Enumerations Enumerator Groups Pages
System Configuration Files system_<device>.c and system_<device>.h

The System Configuration Files system_<device>.c and system_<device>.h provides as a minimum the functions described under System and Clock Configuration. These functions are device specific and need adaptations. In addition, the file might have configuration settings for the device such as XTAL frequency or PLL prescaler settings.

For devices with external memory BUS the system_<device>.c also configures the BUS system.

The silicon vendor might expose other functions (i.e. for power configuration) in the system_<device>.c file. In case of additional features the function prototypes need to be added to the system_<device>.h header file.

# system_Device.c Template File

The system_Device.c Template File for the Cortex-M3 is shown below.

    /**************************************************************************//**
     * @file     system_<Device>.c
     * @brief    CMSIS Cortex-M# Device Peripheral Access Layer Source File for
     *           Device <Device>
     * @version  V3.10
     * @date     23. November 2012
     *
     * @note
     *
     ******************************************************************************/
    /* Copyright (c) 2012 ARM LIMITED

       All rights reserved.
       Redistribution and use in source and binary forms, with or without
       modification, are permitted provided that the following conditions are met:
       - Redistributions of source code must retain the above copyright
         notice, this list of conditions and the following disclaimer.
       - Redistributions in binary form must reproduce the above copyright
         notice, this list of conditions and the following disclaimer in the
         documentation and/or other materials provided with the distribution.
       - Neither the name of ARM nor the names of its contributors may be used
         to endorse or promote products derived from this software without
         specific prior written permission.
       *
       THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS"
       AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE
       IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE
       ARE DISCLAIMED. IN NO EVENT SHALL COPYRIGHT HOLDERS AND CONTRIBUTORS BE
       LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR
       CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF
       SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS
       INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN
       CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE)
       ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE
       POSSIBILITY OF SUCH DAMAGE.
       ---------------------------------------------------------------------------*/

    #include <stdint.h>
    #include "<Device>.h"

    /*----------------------------------------------------------------------------
      DEFINES
     *----------------------------------------------------------------------------*/

    /*----------------------------------------------------------------------------
      Define clocks
     *----------------------------------------------------------------------------*/
    /* ToDo: add here your necessary defines for device initialization
             following is an example for different system frequencies             */
    #define __HSI             ( 6000000UL)
    #define __XTAL            (12000000UL)    /* Oscillator frequency             */
    #define __SYS_OSC_CLK     (    ___HSI)    /* Main oscillator frequency        */

    #define __SYSTEM_CLOCK    (4*__XTAL)

    /*----------------------------------------------------------------------------
      Clock Variable definitions
     *----------------------------------------------------------------------------*/
    /* ToDo: initialize SystemCoreClock with the system core clock frequency value
             achieved after system intitialization.
             This means system core clock frequency after call to SystemInit()    */
    uint32_t SystemCoreClock = __SYSTEM_CLOCK;  /*!< System Clock Frequency (Core Clock)*/

    /*----------------------------------------------------------------------------
      Clock functions
     *----------------------------------------------------------------------------*/
    void SystemCoreClockUpdate (void)            /* Get Core Clock Frequency      */
    {
    /* ToDo: add code to calculate the system frequency based upon the current
             register settings.
             This function can be used to retrieve the system core clock frequeny
             after user changed register sittings.                                */
      SystemCoreClock = __SYSTEM_CLOCK;
    }

    /**
     * Initialize the system
     *
     * @param  none
     * @return none
     *
     * @brief  Setup the microcontroller system.
     *         Initialize the System.
     */
    void SystemInit (void)
    {
    /* ToDo: add code to initialize the system
             do not use global variables because this function is called before
             reaching pre-main. RW section maybe overwritten afterwards.          */
      SystemCoreClock = __SYSTEM_CLOCK;
    }

# system_Device.h Template File

The system_<device>.h header file contains prototypes to access the public functions in the system_<device>.c file. The system_Device.h Template File is shown below.

    /**************************************************************************//**
     * @file     system_<Device>.h
     * @brief    CMSIS Cortex-M# Device Peripheral Access Layer Header File for
     *           Device <Device>
     * @version  V3.10
     * @date     23. November 2012
     *
     * @note
     *
     ******************************************************************************/
    /* Copyright (c) 2012 ARM LIMITED

       All rights reserved.
       Redistribution and use in source and binary forms, with or without
       modification, are permitted provided that the following conditions are met:
       - Redistributions of source code must retain the above copyright
         notice, this list of conditions and the following disclaimer.
       - Redistributions in binary form must reproduce the above copyright
         notice, this list of conditions and the following disclaimer in the
         documentation and/or other materials provided with the distribution.
       - Neither the name of ARM nor the names of its contributors may be used
         to endorse or promote products derived from this software without
         specific prior written permission.
       *
       THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS"
       AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE
       IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE
       ARE DISCLAIMED. IN NO EVENT SHALL COPYRIGHT HOLDERS AND CONTRIBUTORS BE
       LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR
       CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF
       SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS
       INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN
       CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE)
       ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE
       POSSIBILITY OF SUCH DAMAGE.
       ---------------------------------------------------------------------------*/

    #ifndef SYSTEM_<Device>_H   /* ToDo: replace '<Device>' with your device name */
    #define SYSTEM_<Device>_H

    #ifdef __cplusplus
    extern "C" {
    #endif

    #include <stdint.h>

    extern uint32_t SystemCoreClock;     /*!< System Clock Frequency (Core Clock)  */

    /**
     * Initialize the system
     *
     * @param  none
     * @return none
     *
     * @brief  Setup the microcontroller system.
     *         Initialize the System and update the SystemCoreClock variable.
     */
    extern void SystemInit (void);

    /**
     * Update SystemCoreClock variable
     *
     * @param  none
     * @return none
     *
     * @brief  Updates the SystemCoreClock with current core Clock
     *         retrieved from cpu registers.
     */
    extern void SystemCoreClockUpdate (void);

    #ifdef __cplusplus
    }
    #endif

    #endif /* SYSTEM_<Device>_H */