| CMSIS-Driver Version 2.02 Peripheral Interface for Middleware and Application Code

- CMSIS
- CORE
- Driver
- DSP
- RTOS API
- Pack
- SVD

- Main Page
- Usage and Description
- Reference

- All
- Functions
- Typedefs
- Enumerations
- Enumerator
- Macros

- e
- f
- i
- m
- n
- s
- u

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages

### - e -

- ARM_ETH_MAC_Control() : Driver_ETH_MAC.c
- ARM_ETH_MAC_ControlTimer() : Driver_ETH_MAC.c
- ARM_ETH_MAC_GetCapabilities() : Driver_ETH_MAC.c
- ARM_ETH_MAC_GetMacAddress() : Driver_ETH_MAC.c
- ARM_ETH_MAC_GetRxFrameSize() : Driver_ETH_MAC.c
- ARM_ETH_MAC_GetRxFrameTime() : Driver_ETH_MAC.c
- ARM_ETH_MAC_GetTxFrameTime() : Driver_ETH_MAC.c
- ARM_ETH_MAC_GetVersion() : Driver_ETH_MAC.c
- ARM_ETH_MAC_Initialize() : Driver_ETH_MAC.c
- ARM_ETH_MAC_PHY_Read() : Driver_ETH_MAC.c
- ARM_ETH_MAC_PHY_Write() : Driver_ETH_MAC.c
- ARM_ETH_MAC_PowerControl() : Driver_ETH_MAC.c
- ARM_ETH_MAC_ReadFrame() : Driver_ETH_MAC.c
- ARM_ETH_MAC_SendFrame() : Driver_ETH_MAC.c
- ARM_ETH_MAC_SetAddressFilter() : Driver_ETH_MAC.c
- ARM_ETH_MAC_SetMacAddress() : Driver_ETH_MAC.c
- ARM_ETH_MAC_SignalEvent() : Driver_ETH_MAC.c
- ARM_ETH_MAC_Uninitialize() : Driver_ETH_MAC.c
- ARM_ETH_PHY_GetLinkInfo() : Driver_ETH_PHY.c
- ARM_ETH_PHY_GetLinkState() : Driver_ETH_PHY.c
- ARM_ETH_PHY_GetVersion() : Driver_ETH_PHY.c
- ARM_ETH_PHY_Initialize() : Driver_ETH_PHY.c
- ARM_ETH_PHY_PowerControl() : Driver_ETH_PHY.c
- ARM_ETH_PHY_SetInterface() : Driver_ETH_PHY.c
- ARM_ETH_PHY_SetMode() : Driver_ETH_PHY.c
- ARM_ETH_PHY_Uninitialize() : Driver_ETH_PHY.c

### - f -

- ARM_Flash_EraseChip() : Driver_Flash.c
- ARM_Flash_EraseSector() : Driver_Flash.c
- ARM_Flash_GetCapabilities() : Driver_Flash.c
- ARM_Flash_GetInfo() : Driver_Flash.c
- ARM_Flash_GetStatus() : Driver_Flash.c
- ARM_Flash_GetVersion() : Driver_Flash.c
- ARM_Flash_Initialize() : Driver_Flash.c
- ARM_Flash_PowerControl() : Driver_Flash.c
- ARM_Flash_ProgramData() : Driver_Flash.c
- ARM_Flash_ReadData() : Driver_Flash.c
- ARM_Flash_SignalEvent() : Driver_Flash.c
- ARM_Flash_Uninitialize() : Driver_Flash.c

### - i -

- ARM_I2C_Control() : Driver_I2C.c
- ARM_I2C_GetCapabilities() : Driver_I2C.c
- ARM_I2C_GetDataCount() : Driver_I2C.c
- ARM_I2C_GetStatus() : Driver_I2C.c
- ARM_I2C_GetVersion() : Driver_I2C.c
- ARM_I2C_Initialize() : Driver_I2C.c
- ARM_I2C_MasterReceive() : Driver_I2C.c
- ARM_I2C_MasterTransmit() : Driver_I2C.c
- ARM_I2C_PowerControl() : Driver_I2C.c
- ARM_I2C_SignalEvent() : Driver_I2C.c
- ARM_I2C_SlaveReceive() : Driver_I2C.c
- ARM_I2C_SlaveTransmit() : Driver_I2C.c
- ARM_I2C_Uninitialize() : Driver_I2C.c

### - m -

- ARM_MCI_AbortTransfer() : Driver_MCI.c
- ARM_MCI_CardPower() : Driver_MCI.c
- ARM_MCI_Control() : Driver_MCI.c
- ARM_MCI_GetCapabilities() : Driver_MCI.c
- ARM_MCI_GetStatus() : Driver_MCI.c
- ARM_MCI_GetVersion() : Driver_MCI.c
- ARM_MCI_Initialize() : Driver_MCI.c
- ARM_MCI_PowerControl() : Driver_MCI.c
- ARM_MCI_ReadCD() : Driver_MCI.c
- ARM_MCI_ReadWP() : Driver_MCI.c
- ARM_MCI_SendCommand() : Driver_MCI.c
- ARM_MCI_SetupTransfer() : Driver_MCI.c
- ARM_MCI_SignalEvent() : Driver_MCI.c
- ARM_MCI_Uninitialize() : Driver_MCI.c

### - n -

- ARM_NAND_AbortSequence() : Driver_NAND.c
- ARM_NAND_ChipEnable() : Driver_NAND.c
- ARM_NAND_Control() : Driver_NAND.c
- ARM_NAND_DevicePower() : Driver_NAND.c
- ARM_NAND_ExecuteSequence() : Driver_NAND.c
- ARM_NAND_GetCapabilities() : Driver_NAND.c
- ARM_NAND_GetDeviceBusy() : Driver_NAND.c
- ARM_NAND_GetStatus() : Driver_NAND.c
- ARM_NAND_GetVersion() : Driver_NAND.c
- ARM_NAND_Initialize() : Driver_NAND.c
- ARM_NAND_InquireECC() : Driver_NAND.c
- ARM_NAND_PowerControl() : Driver_NAND.c
- ARM_NAND_ReadData() : Driver_NAND.c
- ARM_NAND_SendAddress() : Driver_NAND.c
- ARM_NAND_SendCommand() : Driver_NAND.c
- ARM_NAND_SignalEvent() : Driver_NAND.c
- ARM_NAND_Uninitialize() : Driver_NAND.c
- ARM_NAND_WriteData() : Driver_NAND.c
- ARM_NAND_WriteProtect() : Driver_NAND.c

### - s -

- ARM_SPI_Control() : Driver_SPI.c
- ARM_SPI_GetCapabilities() : Driver_SPI.c
- ARM_SPI_GetDataCount() : Driver_SPI.c
- ARM_SPI_GetStatus() : Driver_SPI.c
- ARM_SPI_GetVersion() : Driver_SPI.c
- ARM_SPI_Initialize() : Driver_SPI.c
- ARM_SPI_PowerControl() : Driver_SPI.c
- ARM_SPI_Receive() : Driver_SPI.c
- ARM_SPI_Send() : Driver_SPI.c
- ARM_SPI_SignalEvent() : Driver_SPI.c
- ARM_SPI_Transfer() : Driver_SPI.c
- ARM_SPI_Uninitialize() : Driver_SPI.c

### - u -

- ARM_USART_Control() : Driver_USART.c
- ARM_USART_GetCapabilities() : Driver_USART.c
- ARM_USART_GetModemStatus() : Driver_USART.c
- ARM_USART_GetRxCount() : Driver_USART.c
- ARM_USART_GetStatus() : Driver_USART.c
- ARM_USART_GetTxCount() : Driver_USART.c
- ARM_USART_GetVersion() : Driver_USART.c
- ARM_USART_Initialize() : Driver_USART.c
- ARM_USART_PowerControl() : Driver_USART.c
- ARM_USART_Receive() : Driver_USART.c
- ARM_USART_Send() : Driver_USART.c
- ARM_USART_SetModemControl() : Driver_USART.c
- ARM_USART_SignalEvent() : Driver_USART.c
- ARM_USART_Transfer() : Driver_USART.c
- ARM_USART_Uninitialize() : Driver_USART.c
- ARM_USBD_DeviceConnect() : Driver_USBD.c
- ARM_USBD_DeviceDisconnect() : Driver_USBD.c
- ARM_USBD_DeviceGetState() : Driver_USBD.c
- ARM_USBD_DeviceRemoteWakeup() : Driver_USBD.c
- ARM_USBD_DeviceSetAddress() : Driver_USBD.c
- ARM_USBD_EndpointConfigure() : Driver_USBD.c
- ARM_USBD_EndpointStall() : Driver_USBD.c
- ARM_USBD_EndpointTransfer() : Driver_USBD.c
- ARM_USBD_EndpointTransferAbort() : Driver_USBD.c
- ARM_USBD_EndpointTransferGetResult() : Driver_USBD.c
- ARM_USBD_EndpointUnconfigure() : Driver_USBD.c
- ARM_USBD_GetCapabilities() : Driver_USBD.c
- ARM_USBD_GetFrameNumber() : Driver_USBD.c
- ARM_USBD_GetVersion() : Driver_USBD.c
- ARM_USBD_Initialize() : Driver_USBD.c
- ARM_USBD_PowerControl() : Driver_USBD.c
- ARM_USBD_ReadSetupPacket() : Driver_USBD.c
- ARM_USBD_SignalDeviceEvent() : Driver_USBD.c
- ARM_USBD_SignalEndpointEvent() : Driver_USBD.c
- ARM_USBD_Uninitialize() : Driver_USBD.c
- ARM_USBH_GetCapabilities() : Driver_USBH.c
- ARM_USBH_GetFrameNumber() : Driver_USBH.c
- ARM_USBH_GetVersion() : Driver_USBH.c
- ARM_USBH_HCI_GetCapabilities() : Driver_USBH.c
- ARM_USBH_HCI_GetVersion() : Driver_USBH.c
- ARM_USBH_HCI_Initialize() : Driver_USBH.c
- ARM_USBH_HCI_Interrupt() : Driver_USBH.c
- ARM_USBH_HCI_PortVbusOnOff() : Driver_USBH.c
- ARM_USBH_HCI_PowerControl() : Driver_USBH.c
- ARM_USBH_HCI_Uninitialize() : Driver_USBH.c
- ARM_USBH_Initialize() : Driver_USBH.c
- ARM_USBH_PipeCreate() : Driver_USBH.c
- ARM_USBH_PipeDelete() : Driver_USBH.c
- ARM_USBH_PipeModify() : Driver_USBH.c
- ARM_USBH_PipeReset() : Driver_USBH.c
- ARM_USBH_PipeTransfer() : Driver_USBH.c
- ARM_USBH_PipeTransferAbort() : Driver_USBH.c
- ARM_USBH_PipeTransferGetResult() : Driver_USBH.c
- ARM_USBH_PortGetState() : Driver_USBH.c
- ARM_USBH_PortReset() : Driver_USBH.c
- ARM_USBH_PortResume() : Driver_USBH.c
- ARM_USBH_PortSuspend() : Driver_USBH.c
- ARM_USBH_PortVbusOnOff() : Driver_USBH.c
- ARM_USBH_PowerControl() : Driver_USBH.c
- ARM_USBH_SignalPipeEvent() : Driver_USBH.c
- ARM_USBH_SignalPortEvent() : Driver_USBH.c
- ARM_USBH_Uninitialize() : Driver_USBH.c